|  |  |
| --- | --- |
| **TASK** | Cherry Picker |
| **HAZARDS** | Flying debris |[ ]  Heat / cold |[ ]  Electricity |[x]
|  | Cuts / laceration |[ ]  Dust |[ ]  Rollover |[x]
|  | Pinch / crush  |[x]  Noise / vibration |[ ]  Plant interaction |[x]
|  | High pressure |[ ]  Falling |[x]  Tip over |[x]
| **PPE REQUIRED** |  |
|  |
| **PRE-START CHECKS** |
| 1. Complete pre-start checks as pe manufacturer’s guidelines.
2. Check the stability of the ground and ensure it can support the weight of the cherry picker.
3. Verify that all safety features, such as guardrails and emergency stop buttons, are functional.
4. Confirm that all controls and systems are operational by performing a test lift and lowering.
 |
|  |
| **SAFE OPERATING PROCEDURE** |
| 1. Ensure personnel are competent and authorized.
2. Ensure personnel are fit for duty and not impaired by drugs or alcohol.
3. Do not use a mobile phone while operating and always wear your seatbelt.
4. Operate at a safe speed and maintain exclusion zones around people, powerlines, and other hazards (use spotters if necessary).
5. Beware of uneven or sloping ground.
6. Use the provided harness and attach to the designated anchor point before ascending.
7. Operate the cherry picker smoothly, avoiding sudden movements or overloading.
8. Lower the platform completely and secure it before exiting the cherry picker.
 |
|  |
| **POST-OPERATION PROCEDURE** |
| 1. Lower the platform to the ground and turn off the cherry picker.
2. Perform a final visual inspection for any damage or debris.
3. Secure the cherry picker and return it to the designated storage area.
4. Report any issues or incidents encountered during operation to the appropriate personnel.
 |